**Basic lapped seam**

**Class - 02**

Basic lapped Seam is a seam in which the raw edges of seam allowances of the fabrics overlap and are stitched in place.

Place the left edge of one fabric parallel to the right edge of the other fabric and stitch along a straight line with a half inch seam allowance. Seams should be back-stitched at the beginning and end to prevent them from coming undone at these ends. Basic lapped seam used for fabric don’t fry, such as leather,wool,felt,viny.

**Welted lapped seam**

**Class - 02**

Decorative lapped seam with dimension created by a narrow seam allowance caught between the garment and a winder seam allowance by topstitching.

1) Place both fabric pieces right sides up and overlap the edge by the seam allowance.

2) Draw a line or pin a guideline along the seam allowances. Run a straight stitch along the edge of the upper piece of fabric 3) Turn the joined fabric over to the wrong side and sew another line of straight stitching along the other side of the lapped seam.

4) Press the seam with a pressing cloth.

A welted lapped seam is also frequently used for jeans, as it is very strong.